|RECORD=BOM|VERSION=2|FILENAME=E:\Altium\Projects\Viscometer\Thermostat\Thermostat.BomDoc|KIND=ALTIUM_DESIGNER_LIVEBOM|DATE=14.06.2024|TIME=11:53:41|CURRENCY=USD|PRODUCTIONQUANTITY=1|PERUNITTARGETPRICE=0|PERUNITACTUALPRICE=0
|RECORD=GeneralOptions|OPENEXPORTED=False|ADDTOPROJECT=False|FORCEFIT=False|NOTFITTED=False|TEMPLATEFILENAME=|BATCHMODE=0|SUPPLIERPRODQTY=0|SUPPLIERAUTOQTY=False|SUPPLIERUSECACHEDPRICING=False|SUPPLIERCURRENCY=|SOLUTIONSPERITEM=1|SUPPLIERSPERSOLUTION=1|DISPLAYTOTALROW=False|DISPLAYSUBTOTALSFORGROUPS=False|INCLUDEPCBPARAMETERS=False|INCLUDEDBPARAMETERS=False|INCLUDEVAULTPARAMETERS=False|INCLUDECLOUDPARAMETERS=False|INCLUDEDOCUMENTPARAMETERS=False|FILTEROUTRISKYSOLUTIONS=True|DESIGNATORGROUPING=No
|RECORD=SortOrderOptions|SORTORDER=
|RECORD=GroupOrderOptions|GROUPORDER=
|RECORD=VisibleOrderOptions|VISIBLEORDER=Designator=126!Name=134!Comment=134!Description=81!Footprint=70!Quantity=67
|RECORD=VisibleOrderOptions2|BASEVIEW=Designator=126!Name=134!Comment=134!Description=81!Footprint=70!Quantity=67|FLATVIEW=Line #=-1!Comment=-1!Description=-1!Designator=-1!Manufacturer 1=101!Manufacturer Part Number 1=170!Manufacturer Lifecycle 1=147!Supplier 1=74!Supplier Part Number 1=143!Supplier Unit Price 1=127!Supplier Subtotal 1=120|CONSOLIDATEDVIEW=Line #=-1!Comment=-1!Description=-1!Designator=-1!Quantity=-1!Manufacturer 1=101!Manufacturer Part Number 1=170!Manufacturer Lifecycle 1=147!Supplier 1=74!Supplier Part Number 1=143!Supplier Unit Price 1=127!Supplier Subtotal 1=120
|RECORD=CustomColumns|CUSTOMCOLUMNS=
|RECORD=ColumnsAliases|COLUMNSALIASES=Comment=Name
|RECORD=FilterOptions|FILTER=
|RECORD=CheckGroupCompParamsOptions|CHECKGROUPCOMPPARAMS=Comment=0,Description=0,Value=0,Footprint=1
|RECORD=ManufacturerLinkOptions|MANUFACTURERLINKPARAMETERS=
|RECORD=FavoriteSuppliers|SUPPLIERS=|USESUPPLIERORDER=False
|RECORD=CheckOptions|CHECKLEVELS=
|RECORD=LineNumberingOptions|STARTVALUE=|INCREMENT=
|RECORD=Catalog|DBLINKFILEPATH=
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\CAP_1210|DESIGNITEMID=CAP_1210|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Capacitor Ceramic 1210|USERCOMMENTS=22uF, 25V|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="22uF, 25V","Capacitor Ceramic 1210"|COMPONENTPARAMETERS="Comment=22uF, 25V","Component Kind=Standard","Description=Capacitor Ceramic 1210",Footprint=CAP_1210,Group=Capacitor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=CAP_1210",Name=CL32A226KAJNNNE,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Ceramic 1210","Value=22uF, 25V"|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\CAP_0603|DESIGNITEMID=CAP_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Capacitor Ceramic 0603|USERCOMMENTS=56pF, 25V|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="56pF, 25V","Capacitor Ceramic 0603"|COMPONENTPARAMETERS="Comment=56pF, 25V","Component Kind=Standard","Description=Capacitor Ceramic 0603",Footprint=CAP_0603,Group=Capacitor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=CAP_0603",Name=,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Ceramic 0603","Value=56pF, 25V"|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\CAP_0603|DESIGNITEMID=CAP_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Capacitor Ceramic 0603|USERCOMMENTS=10nF, 25V|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="10nF, 25V","Capacitor Ceramic 0603"|COMPONENTPARAMETERS="Comment=10nF, 25V","Component Kind=Standard","Description=Capacitor Ceramic 0603",Footprint=CAP_0603,Group=Capacitor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=CAP_0603",Name=,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Ceramic 0603","Value=10nF, 25V"|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\BZT52C4V7S|DESIGNITEMID=BZT52C4V7S|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Zener Diode, Diodes, 200mW 4.7V|USERCOMMENTS=BZT52C9V1S|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=BZT52C9V1S,"Zener Diode, Diodes, 200mW 4.7V"|COMPONENTPARAMETERS=Comment=BZT52C9V1S,"Component Kind=Standard",ComponentLink1Description=Datasheet,ComponentLink1URL=https://eu.mouser.com/datasheet/2/115/DIOD_S_A0003132830_1-2542423.pdf,"Description=Zener Diode, Diodes, 200mW 4.7V",Footprint=SOD323,Group=Diodes,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=BZT52C4V7S",Name=BZT52C9V1S,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,SubGroup=Zener|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\FFC3B11-10-T|DESIGNITEMID=FFC3B11-10-T|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=FFC, 1mm pitch, 10 pins Side Flat Flexible Cable Connector|USERCOMMENTS=FFC3B11-10-T|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="FFC, 1mm pitch, 10 pins Side Flat Flexible Cable Connector",FFC3B11-10-T|COMPONENTPARAMETERS=Alternative=DS1020-07-10VB8A-R,Comment=FFC3B11-10-T,"Component Kind=Standard",ComponentLink1Description=Datasheet,ComponentLink1URL=https://gct.co/files/drawings/ffc3b07.pdf?v=a58fe42b-0664-4f3e-9680-4f57a179bb65,"ComponentLink2Description=Datasheet 1",ComponentLink2URL=https://www.promelec.ru/fs/sources/37/ff/96/31/4248e2d54346a1de41d05af9.pdf,"Description=FFC, 1mm pitch, 10 pins Side Flat Flexible Cable Connector",Footprint=FFC3B11-10-T_GCT,Group=Connector,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=FFC3B11-10-T",Name=FFC3B11-10-T,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,SubGroup=FFC|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\TIP32|DESIGNITEMID=TIP32|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=BJT, Onsemi, PNP transistor, Vceo=-40V, Ice=-3A, hfe=10-50|USERCOMMENTS=TIP32|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="BJT, Onsemi, PNP transistor, Vceo=-40V, Ice=-3A, hfe=10-50",TIP32|COMPONENTPARAMETERS=Comment=TIP32,"Component Kind=Standard",ComponentLink1Description=Datasheet,ComponentLink1URL=https://www.onsemi.com/pdf/datasheet/tip32c-d.pdf,"Description=BJT, Onsemi, PNP transistor, Vceo=-40V, Ice=-3A, hfe=10-50",Footprint=TO-220-3_planar,Group=SwitchDevice.BJT,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=TIP32",Name=TIP32,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,SubGroup=PNP|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\2N7002|DESIGNITEMID=2N7002|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=MOSFET, Nexperia, N-channel field effect transistor, Vds 60V, Id  300mA, -65/+150C|USERCOMMENTS=2N7002|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=2N7002,"MOSFET, Nexperia, N-channel field effect transistor, Vds 60V, Id  300mA, -65/+150C"|COMPONENTPARAMETERS=Comment=2N7002,"Component Kind=Standard",ComponentLink1Description=Datasheet,ComponentLink1URL=https://assets.nexperia.com/documents/data-sheet/2N7002.pdf,"Description=MOSFET, Nexperia, N-channel field effect transistor, Vds 60V, Id  300mA, -65/+150C",Footprint=SOT-23-3,Group=MOSFET,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=2N7002",Name=2N7002,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,SubGroup=MOSFET-N|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=820|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=820,"Resistor 0603"|COMPONENTPARAMETERS=Comment=820,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-07820RL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=820|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=9.1k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=9.1k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=9.1k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-079K1L,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=9.1k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\3296P-1-471|DESIGNITEMID=3296P-1-471|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Potentiometer, Bourns, 470 Ohms 0.5W, Through Hole Trimmer Potentiometer Cermet 25 Turn Side Adjustment|USERCOMMENTS=470|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=470,"Potentiometer, Bourns, 470 Ohms 0.5W, Through Hole Trimmer Potentiometer Cermet 25 Turn Side Adjustment"|COMPONENTPARAMETERS=Comment=470,"Component Kind=Standard","Description=Potentiometer, Bourns, 470 Ohms 0.5W, Through Hole Trimmer Potentiometer Cermet 25 Turn Side Adjustment",Footprint=TRIM_3296P-1-105,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=3296P-1-471",Name=3296P-1-471,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Trimmer Potentiometer",Value=470|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=30k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=30k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=30k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-0730KL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=30k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=1k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=1k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=1k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-071KL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=1k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=200|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=200,"Resistor 0603"|COMPONENTPARAMETERS=Comment=200,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-07200RL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=200|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=47k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=47k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=47k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-0747KL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=47k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=2k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=2k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=2k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-072KL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=2k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=1M|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=1M,"Resistor 0603"|COMPONENTPARAMETERS=Comment=1M,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-071ML,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=1M|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=91k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=91k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=91k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-0791KL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=91k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=10k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=10k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=10k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-0710KL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=10k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=DNP|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=DNP,"Resistor 0603"|COMPONENTPARAMETERS=Comment=DNP,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=DNP,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=DNP|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=6k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=6k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=6k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-076KL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=6k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\RES_0603|DESIGNITEMID=RES_0603|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Resistor 0603|USERCOMMENTS=100k|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=100k,"Resistor 0603"|COMPONENTPARAMETERS=Comment=100k,"Component Kind=Standard","Description=Resistor 0603",Footprint=RES_0603,Group=Resistor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=RES_0603",Name=RC0603FR-07100KL,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Chip 0603",Value=100k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\LM358|DESIGNITEMID=LM358|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=OpAmp, TI, dual, low power, supply voltage 3/32V|USERCOMMENTS=LM358|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=LM358,"OpAmp, TI, dual, low power, supply voltage 3/32V"|COMPONENTPARAMETERS=Comment=LM358,"Component Kind=Standard",ComponentLink1Description=Datasheet,ComponentLink1URL=https://www.ti.com/lit/ds/snosbt3j/snosbt3j.pdf?ts=1687863016311,"Description=OpAmp, TI, dual, low power, supply voltage 3/32V",Footprint=SO-8,Group=OpAmp,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=LM358",Name=LM358,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\TMP116NAIDRVR|DESIGNITEMID=TMP116NAIDRVR|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Temperature sensor, TI, 0.2C Accurate Digital I2C With NV Memory 6-WSON -55 to 125|USERCOMMENTS=TMP116AIDRVR|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="Temperature sensor, TI, 0.2C Accurate Digital I2C With NV Memory 6-WSON -55 to 125",TMP116AIDRVR|COMPONENTPARAMETERS=Comment=TMP116AIDRVR,"Component Kind=Standard",ComponentLink1Description=Datasheet,ComponentLink1URL=https://www.ti.com/lit/ds/symlink/tmp116.pdf?ts=1713895163789&ref_url=https%253A%252F%252Fwww.google.com%252F,"Description=Temperature sensor, TI, 0.2C Accurate Digital I2C With NV Memory 6-WSON -55 to 125",Footprint=SON65P200X200X80-7N,Group=Sensor,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=TMP116NAIDRVR","MF=Texas Instruments",Name=TMP116AIDRVR,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"SubGroup=Temperature sensor"|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=SistematicsLib.IntLib\SN74LVC1G74DCU|DESIGNITEMID=SN74LVC1G74DCU|ITEMSOURCE=SistematicsLib.IntLib|STATUS=Unknown|DESCRIPTION=Flip-Flop, TI, Single Positive-Edge-Triggered D-Type Flip-Flop with Clear and Preset, 1.65-V to 5.5-V|USERCOMMENTS=SN74LVC1G74DCUR|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="Flip-Flop, TI, Single Positive-Edge-Triggered D-Type Flip-Flop with Clear and Preset, 1.65-V to 5.5-V",SN74LVC1G74DCUR|COMPONENTPARAMETERS=Comment=SN74LVC1G74DCUR,"Component Kind=Standard",ComponentLink1Description=Datasheet,ComponentLink1URL=https://www.ti.com/lit/ds/symlink/sn74lvc1g74.pdf,"Description=Flip-Flop, TI, Single Positive-Edge-Triggered D-Type Flip-Flop with Clear and Preset, 1.65-V to 5.5-V",Footprint=SO-8_P0.5_DCU,Group=Logic,"Ibis Model=","Library Name=SistematicsLib.IntLib","Library Reference=SN74LVC1G74DCU",Name=SN74LVC1G74DCUR,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,SubGroup=Flip-Flop|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
